EXTERNAL PORTS
These are the external ports defined in the MHS file.
Attributes Key The attributes are obtained from the SIGIS and IOB_STATE parameters set on the PORT in the MHS file CLK indicates Clock ports, (SIGIS = CLK) INTR indicates Interrupt ports,(SIGIS = INTR) RESET indicates Reset ports, (SIGIS = RST) BUF or REG Indicates ports that instantiate or infer IOB primitives, (IOB_STATE = BUF or REG)
# | NAME | DIR | [LSB:MSB] | SIG | ATTRIBUTES
| fpga_0_RS232_Uart_RX_pin | I | 1 | fpga_0_RS232_Uart_RX |
| fpga_0_RS232_Uart_TX_pin | O | 1 | fpga_0_RS232_Uart_TX |
| fpga_0_LEDs_4Bit_GPIO_IO_pin | IO | 0:3 | fpga_0_LEDs_4Bit_GPIO_IO |
| fpga_0_LEDs_Positions_GPIO_IO_pin | IO | 0:4 | fpga_0_LEDs_Positions_GPIO_IO |
| fpga_0_SysACE_CompactFlash_SysACE_CLK_pin | I | 1 | fpga_0_SysACE_CompactFlash_SysACE_CLK |
| fpga_0_SysACE_CompactFlash_SysACE_MPA_pin | O | 6:1 | fpga_0_SysACE_CompactFlash_SysACE_MPA |
| fpga_0_SysACE_CompactFlash_SysACE_MPD_pin | IO | 15:0 | fpga_0_SysACE_CompactFlash_SysACE_MPD |
| fpga_0_SysACE_CompactFlash_SysACE_CEN_pin | O | 1 | fpga_0_SysACE_CompactFlash_SysACE_CEN |
| fpga_0_SysACE_CompactFlash_SysACE_OEN_pin | O | 1 | fpga_0_SysACE_CompactFlash_SysACE_OEN |
| fpga_0_SysACE_CompactFlash_SysACE_WEN_pin | O | 1 | fpga_0_SysACE_CompactFlash_SysACE_WEN |
| fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin | I | 1 | fpga_0_SysACE_CompactFlash_SysACE_MPIRQ |  |  | # | NAME | DIR | [LSB:MSB] | SIG | ATTRIBUTES
| fpga_0_SRAM_Mem_A_pin | O | 9:29 | fpga_0_SRAM_Mem_A |
| fpga_0_SRAM_Mem_BEN_pin | O | 0:3 | fpga_0_SRAM_Mem_BEN |
| fpga_0_SRAM_Mem_WEN_pin | O | 1 | fpga_0_SRAM_Mem_WEN |
| fpga_0_SRAM_Mem_DQ_pin | IO | 0:31 | fpga_0_SRAM_Mem_DQ |
| fpga_0_SRAM_Mem_OEN_pin | O | 0:0 | fpga_0_SRAM_Mem_OEN |
| fpga_0_SRAM_Mem_CEN_pin | O | 0:0 | fpga_0_SRAM_Mem_CEN |
| fpga_0_SRAM_Mem_ADV_LDN_pin | O | 1 | fpga_0_SRAM_Mem_ADV_LDN |
| fpga_0_SRAM_CLOCK | O | 1 | sys_clk_s |
| sys_clk_pin | I | 1 | dcm_clk_s | CLK
| sys_rst_pin | I | 1 | sys_rst_s | RESET